{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["定制柜"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"定制柜","index":0,"n_rows":63,"n_cols":8,"rows_kept":63,"merged":[[0,0,0,7]]}
["郁南县中医院易地新建项目（二三期）定制柜清单"]
["序号","类型","规格","计量单位","暂估工程量","备注","单价（元）","总价（元）"]
[1,"医疗综合楼病房衣柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","㎡",879.79]
[2,"医疗综合楼病房衣柜拉手","斜切工艺拉手","个",1664]
[3,"医疗综合楼病房电视柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","㎡",1658]
[4,"医疗综合楼病房电视柜台面","15mm厚白色石英石","m",874.2]
[5,"医疗综合楼病房电视柜拉手","斜切工艺拉手","个",832]
[6,"医疗综合楼中医治疗室地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",36.14,"不含盆和龙头"]
[7,"医疗综合楼中医治疗室地柜台面","15mm厚白色石英石","m",36.14]
[8,"医疗综合楼中医治疗室地柜拉手","斜切工艺拉手","个",84]
[9,"医疗综合楼中医治疗室吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",23.4]
[10,"医疗综合楼护士站后面矮柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",90.66,"不含盆和龙头"]
[11,"医疗综合楼护士站后面矮柜台面","15mm厚白色石英石","m",90.66]
[12,"医疗综合楼护士站后面矮柜拉手","斜切工艺拉手","个",196]
[13,"医疗综合楼护士站导医台","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",127.5]
[14,"医疗综合楼护士站导医台台面","15mm厚白色石英石","m",127.5]
[15,"医疗综合楼护士站导医台抽屉","国产三节轨","个",100]
[16,"医疗综合楼更衣室","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","㎡",360.79]
[17,"医疗综合楼更衣室柜门锁","锌合金锁芯","个",590]
[18,"医疗综合楼配药房地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",90.4,"不含盆和龙头"]
[19,"医疗综合楼配药房地柜台面","15mm厚白色石英石","m",90.4]
[20,"医疗综合楼配药房地柜拉手","斜切工艺拉手","个",176]
[21,"医疗综合楼配药房地柜抽屉","国产三节轨","个",68]
[22,"医疗综合楼配药房吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",40.8]
[23,"医疗综合楼茶水配餐室地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",40.26,"不含盆和龙头"]
[24,"医疗综合楼茶水配餐室地柜台面","15mm厚白色石英石","m",40.26]
[25,"医疗综合楼茶水配餐室地柜拉手","斜切工艺拉手","个",42]
[26,"医疗综合楼处置室地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",33.24,"不含盆和龙头"]
[27,"医疗综合楼处置室地柜台面","15mm厚白色石英石","m",33.24]
[28,"医疗综合楼处置室拉手","斜切工艺拉手","个",54]
[29,"医疗综合楼处置室吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":10.8,"d":"10.80"}]
[30,"医疗综合楼污洗打包间地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":20.4,"d":"20.40"},"不含盆和龙头"]
[31,"医疗综合楼污洗打包间地柜台面","15mm厚白色石英石","m",{"v":20.4,"d":"20.40"}]
[32,"医疗综合楼污洗打包间地柜拉手","斜切工艺拉手","个",{"v":39,"d":"39.00"}]
[33,"医疗综合楼污洗打包间吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":20.4,"d":"20.40"}]
[34,"感染楼病房衣柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","㎡",161.58]
[35,"感染楼病房衣柜拉手","斜切工艺拉手","个",{"v":144,"d":"144.00"}]
[36,"感染楼病房电视柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","㎡",314.64]
[37,"感染楼病房电视柜台面","15mm厚白色石英石","m",{"v":116.3,"d":"116.30"}]
[38,"感染楼病房电视柜拉手","斜切工艺拉手","个",{"v":72,"d":"72.00"}]
[39,"感染楼中医治疗室地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",7.05,"不含盆和龙头"]
[40,"感染楼中医治疗室地柜台面","15mm厚白色石英石","m",7.05]
[41,"感染楼中医治疗室地柜拉手","斜切工艺拉手","个",{"v":12,"d":"12.00"}]
[42,"感染楼中医治疗室吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":5.4,"d":"5.40"}]
[43,"感染楼护士站后面矮柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":12.6,"d":"12.60"},"不含盆和龙头"]
[44,"感染楼护士站后面矮柜台面","15mm厚白色石英石","m",{"v":12.6,"d":"12.60"}]
[45,"感染楼护士站后面矮柜拉手","斜切工艺拉手","个",{"v":24,"d":"24.00"}]
[46,"感染楼护士站导医台","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",29.51]
[47,"感染楼护士站导医台台面","15mm厚白色石英石","m",29.51]
[48,"感染楼护士站导医台抽屉","国产三节轨","个",{"v":20,"d":"20.00"}]
[49,"感染楼配药房地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",12.63,"不含盆和龙头"]
[50,"感染楼配药房地柜台面","15mm厚白色石英石","m",12.63]
[51,"感染楼配药房地柜拉手","斜切工艺拉手","个",{"v":24,"d":"24.00"}]
[52,"感染楼配药房地柜抽屉","国产三节轨","个",{"v":12,"d":"12.00"}]
[53,"感染楼配药房吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",10.41]
[54,"感染楼茶水配餐室地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",11.07,"不含盆和龙头"]
[55,"感染楼茶水配餐室地柜台面","15mm厚白色石英石","m",11.07]
[56,"感染楼茶水配餐室地柜拉手","斜切工艺拉手","个",{"v":15,"d":"15.00"}]
[57,"感染楼茶水配餐室吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",11.07]
[58,"感染楼治疗室地柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":3.6,"d":"3.60"},"不含盆和龙头"]
[59,"感染楼治疗室地柜台面","15mm厚白色石英石","m",{"v":3.6,"d":"3.60"}]
[60,"感染楼治疗室地柜拉手","斜切工艺拉手","个",{"v":6,"d":"6.00"}]
[61,"感染楼治疗室吊柜","1.柜身材质：双饰面多层实木，背板：多层实木板材（9mm）\n2.门板材质：双饰面多层实木\n3.工艺标准：封边标准采用PUR封边\n4.固装冷轧钢液压缓冲铰链\n5.定制家具板材环保符合国家现行标准","m",{"v":3.6,"d":"3.60"}]